**Pinout of 7-Segment display**

Because PORTC didn’t have enough pins, I fittet 6 on PB2 and didn’t connect the dot on the

7

6

5

4

3

2

1

0

1st Digit.

0 is connected

To PC0/PD0

An so on